EP3600 Portable Power Station Specifications

GENERAL INFO
	Model
	EP3600iL
	EP3600B(Extra Battery)

	Dimensions/Net Weight
	555X430X420mm, 45kg
	555X415X345mm, 37kg

	Battery
	LiFePO4, 3430Wh, 67Ah(51.2V), 5000 cycles to 80%+capacity

	Operating Temperature
	Discharging Temperature: -20℃~50℃, Charging Temperature: 0℃~45℃

	Transfer Time
	≤10ms
	N/A

	LED
	20W

	Interactive Interface
	LCD Panel / APP
	LCD Panel

	Optional Function
	AC Output Parallel / Wind Charging

/ EV Charger Output / Driving Charger / DC Charger
	Solar Charging / DC Quick Charger

	Protection Grade
	Unit IP53 / Battery Pack IP66
	Unit IP53 / Battery Pack IP66


OUTPUT

	AC Output

(10A/16A/20A×4)

+

(32A/50A×1 For Parallel Output) 

+

(50A×1 For EV Charger AC Output)
	Rated Power
	3600W / VA
	N/A

	
	Peak Power
	7200W / VA
	N/A

	
	Output Waveform
	Pure-Sine Wave, THD<3%
	N/A

	
	Rated Voltage
	100/110/120V, 220/230/240V
	N/A

	
	Rated Frequency
	50/60Hz
	N/A

	DC Output
	XT90 (×1)
	12V/30A
	N/A

	
	Cigarette Lighter Port(×1)
	12V/10A
	N/A

	
	5521 Port(×2)
	12V/6A
	N/A

	USB Output
	USB(×2)
	5V/3.1A
	N/A

	
	QC3.0(×2)
	QC3.0(5V/3.4A, 9V/2A, 12V/1.5A)
	N/A

	
	Type-C(×2)
	PD140W (5V/3A, 9V/3A, 12V/3A, 15V/3A, 20V/5A, 28V/5A)
	N/A

	Wireless Output
	2×5~15W
	N/A


CHARGING INPUT

	Model
	EP3600iL
	EP3600B

(Extra Battery)

	AC
	Wall Outlet & AC Generator
	220~240VAC
	Max. 3000W, 1.2 hours fully charged
	N/A

	
	
	100~120VAC
	Max. 1800W, 2 hours fully charged
	N/A

	Solar
	MPPT Control System
	12~150VDC, Max. 1600~2400W,
2.5 hours fully charged
	12~150VDC, Max. 1200W,

3.2 hours fully charged(1)

	Driving Charging(1)
	Driving Charger With Standard Output Plug
	58.4VDC MAX, Max. 800W,
5 hours fully charged
	N/A

	DC(1)
	DC Charger With Car Cigarette Lighter Input Plug
	12~30V, Max.75W,

55 hours fully charged
	N/A

	Wind(1)
	Wind Charger Inside
	100VAC MAX, Max. 800W,
5 hours fully charged
	N/A

	DC Quick

(1)
	DC Quick Charger
	N/A
	58.4VDC MAX, Max. 3500W,

1.2 hours fully charged


ADD-ONS(Sold Separately)
	EP3600B Extra Battery
	51.2V 3430Wh, Up to 31 units(Total 109kWh)

	SE Series Smart Inverter Generator
	100~240VAC, Max. 1.8~3kW

	DW Series Wind Turbine
	100VAC MAX, Max. 800W

	DSF/DS Series Solar Panels
	41V/82V, Max. 1200~1600W

	DVC Series EV Charging Gun
	100~240VAC, Max. 7200W

	DDC Series Driving Charger
	58.4VDC MAX, Max. 800W

	DDC Series DC Charger
	58.4VDC MAX, Max. 75W

	DAC Series DC Quick Charger
	58.4VDC MAX, Max. 3500W


 NOTE  

(1).All these charging input functions are optional. The Solar charger & DC quick charger for Extra Battery and the Driving charger & DC charger & Wind charger for main unit are optional equipment, which can charge the power station at the same time.
(2).EP3600iL can support AC out parallel function(optional). Two EP3600iL that have the same rated voltage and frequency can be operated in parallel to increase the total available output power reach 7.2 kW.
(3).Whether the product can be charged or discharged depends on the actual temperature of the battery pack. The maximum charging or discharging power is related to the ambient temperature and SOC of battery.
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