EP5000iL Portable Power Station Specifications

GENERAL INFO
	Model
	EP5000iL

	Dimensions/Net Weight
	555X430X420mm, 50kg

	Battery
	LiFePO4, 3430Wh, 67Ah(51.2V), 5000 cycles to 80%+capacity

	Operating Temperature
	Discharging Temperature: -20℃~50℃, Charging Temperature: 0℃~45℃

	Transfer Time
	≤10ms

	LED
	20W

	Interactive Interface
	LCD Panel / APP

	Optional Function
	AC Output Parallel / Wind Charging

/ EV Charger Output / Driving Charger / DC Charger

	Protection Grade
	Unit IP53 / Battery Pack IP66


OUTPUT

	AC Output

(10A/16A/20A×4)

+

(32A/50A×1 For Parallel Output) 

+

(50A×1 For EV Charger AC Output)
	Rated Power
	5000W / VA

	
	Peak Power
	10000W / VA

	
	Output Waveform
	Pure-Sine Wave, THD<3%

	
	Single-phase Rated Voltage
	220/230/240V

	
	Split-phase Rated Voltage
	100/200V, 110/220V, 120/240V

	
	Rated Frequency
	50/60Hz

	DC Output
	XT90 (×1)
	12V/30A

	
	Cigarette Lighter Port(×1)
	12V/10A

	
	5521 Port(×2)
	12V/6A

	USB Output
	USB(×2)
	5V/3.1A

	
	QC3.0(×2)
	QC3.0(5V/3.4A, 9V/2A, 12V/1.5A)

	
	Type-C(×2)
	PD140W (5V/3A, 9V/3A, 12V/3A, 15V/3A, 20V/5A, 28V/5A)

	Wireless Output
	2×5~15W


CHARGING INPUT

	AC
	Wall Outlet & AC Generator
	Single-phase
	Max. 3000W, 1.2 hours fully charged

	
	
	Split-phase
	Max. 1700W, 2 hours fully charged

	Solar
	MPPT Control System
	Single-phase
	12~150VDC, Max. 1200W, 3 hours fully charged

	
	
	Split-phase
	12~150VDC, Max. 1200W, 3 hours fully charged

	Driving Charging(1)
	Driving Charger With Standard Output Plug
	58.4VDC MAX, Max. 800W, 5 hours fully charged

	DC(1)
	Car Cigarette Lighter Port
	12~30V, 8A MAX, Max. 200W, 18 hours fully charged

	Wind(1)
	Wind Charger Inside
	100VAC MAX, Max. 800W, 5 hours fully charged


ADD-ONS(Sold Separately)
	EP3600B Extra Battery
	51.2V 3430Wh, Up to 31 units(Total 109kWh)

	SE Series Smart Inverter Generator
	100~240VAC, Max. 1.8~3kW

	DW Series Wind Turbine
	100VAC MAX, Max. 800W

	DSF/DS Series Solar Panels
	41V/82V, Max. 1200~1600W

	DVC Series EV Charging Gun
	100~240VAC, Max. 7200W

	DDC Series Driving Charger
	58.4VDC MAX, Max. 800W


 NOTE  

(1).All these charging input functions are optional. The Driving charger & DC charging cable & Wind charger are optional equipment, which can charge the power station at the same time.
(2).EP5000iL can support AC out parallel function(optional). Two EP5000iL that have the same rated voltage and frequency can be operated in parallel to increase the total available output power reach 10 kW.
(3).Whether the product can be charged or discharged depends on the actual temperature of the battery pack. The maximum charging or discharging power is related to the ambient temperature and SOC of battery.
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