EP6000 Portable Power Station Specifications

GENERAL INFO
	Model
	EP6000iLS
	EP6000B(Extra Battery)

	Dimensions/Net Weight
	610X560X500mm, 70kg
	610X510X370mm, 55kg

	Battery
	LiFePO4, 5376Wh, 105Ah(51.2V), 5000 cycles to 80%+capacity

	Operating Temperature
	Discharging Temperature: -20℃~50℃, Charging Temperature: 0℃~45℃

	Transfer Time
	≤10ms
	N/A

	LED
	20W

	Interactive Interface
	LCD Panel / APP
	LCD Panel

	Optional Function
	EV Charger Output / Driving Charger / DC Charger
	Solar Charging / DC Quick Charger

	Protection Grade
	Unit IP53 / Battery Pack IP66
	Unit IP53 / Battery Pack IP66


OUTPUT

	AC Output

(10A/16A/20A/30A

×2)

+

(32A/50A×1 ) 

+

(50A×1 For EV Charger AC Output)
	Rated Power
	6000W / VA @120~240V
5500W / VA @110V

5000W / VA @100V
	N/A

	
	Peak Power
	12000W / VA @120~240V

11000W / VA @110V

10000W / VA @100V
	N/A

	
	Output Waveform
	Pure-Sine Wave, THD<3%
	N/A

	
	Single-phase Rated Voltage
	220/230/240V
	N/A

	
	Split-phase Rated Voltage
	100/200V, 110/220V, 120/240V
	N/A

	
	Rated Frequency
	50/60Hz
	N/A

	DC Output
	Cigarette Lighter Port(×1)
	12V/10A
	N/A

	USB Output
(Optional)
	USB(×2)
	5V/3.1A
	N/A

	
	QC3.0(×1)
	QC3.0(5V/3.4A, 9V/2A, 12V/1.5A)
	

	
	Type-C(×1)
	PD60W(5V/3A, 9V/3A, 12V/3A, 15V/3A, 20V/3A)
	


CHARGING INPUT

	Model
	EP6000iLS
	EP6000B

(Extra Battery)

	AC

(16A/32A Dual Input)
	Wall Outlet & AC Generator
	Single-phase
	Max. 3600W / 5500W, 1.7/1.1 hours fully charged
	N/A

	
	
	Split-phase
	Max. 1700W / 5500W, 3.5/1.1 hours fully charged
	N/A

	Solar
	MPPT Control System
	Single-phase
	80~450VDC 27A MAX, Max. 5500W, 1.1 hours fully charged
	12~150VDC, Max. 1200W,

5 hours fully charged(1)

	
	
	Split-phase
	12~150VDC 30A MAX, Max. 3000W, 2 hours fully charged
	

	Driving Charging(1)
	Driving Charger With Standard Output Plug
	58.4VDC MAX, Max. 800W, 7 hours fully charged
	N/A

	DC(1)
	DC Charger With Car Cigarette Lighter Input Plug
	12~30V, Max.75W,

80 hours fully charged
	N/A

	DC Quick

(1)
	DC Quick Charger
	N/A
	58.4VDC MAX, Max. 3500W,

2 hours fully charged


ADD-ONS(Sold Separately)
	EP6000B Extra Battery
	51.2V 5376Wh, Up to 31 units(Total 172kWh)

	SE Series Smart Inverter Generator
	100~240VAC, Max. 1.8/3.7kW

	DSF/DS Series Solar Panels
	41V/82V, Max. 5500W

	DVC Series EV Charging Gun
	100~240VAC, Max. 6000W

	DDC Series Driving Charger
	58.4VDC MAX, Max. 800W

	DDC Series DC Charger
	58.4VDC MAX, Max. 75W

	DAC Series DC Quick Charger
	58.4VDC MAX, Max. 3500W


 NOTE  

(1).All these charging input functions are optional. The Solar charger & DC quick charger for Extra Battery and the Driving charger & DC charger for main unit are optional equipment, which can charge the power station at the same time.
(2).Whether the product can be charged or discharged depends on the actual temperature of the battery pack. The maximum charging or discharging power is related to the ambient temperature and SOC of battery.
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