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  苏州德锐朗智能科技有限公司     Suzhou DriveLong Intelligence Technology Co., Ltd.

CP1200iL Portable Power Station Specifications

GENERAL INFO
	Model
	CP1200iL

	Dimensions/Net Weight
	565X352X246mm, 28kg

	Battery
	LiFePO4, 2048Wh, 80Ah(25.6V), 5000 cycles to 80%+capacity

	Operating Temperature
	Discharging Temperature: -20℃~50℃, Charging Temperature: 0℃~45℃

	Transfer Time
	≤10ms

	Interactive Interface
	LCD Panel / APP

	Protection Grade
	IP65


OUTPUT

	AC Output
	Rated Power
	1200W / VA

	
	Peak Power
	2400W / VA

	
	Output Waveform
	Pure-Sine Wave, THD<3%

	
	Rated Voltage
	100/110/120V, 220/230/240V

	
	Rated Frequency
	50/60Hz

	DC Output
	5521 Port(×2)
	12V/6A

	USB Output
	QC3.0(×1)
	QC3.0(5V/3.4A, 9V/2A, 12V/1.5A)

	
	Type-C(×1)
	PD60W(5V/3A, 9V/3A, 12V/3A, 15V/3A, 20V/3A)


CHARGING INPUT

	AC
	Wall Outlet & AC Generator
	Max. 1000W, 2 hours fully charged

	Solar
	MPPT Control System
	12~75VDC, 12A MAX, Max. 400W, 5 hours fully charged

	DC(1)
	Car Cigarette Lighter Port
	12~30V, 8A MAX, Max.200W, 11 hours fully charged

	Driving Charging(1)
	Driving Charger With Standard Output Plug
	29.2VDC MAX, Max.800W, 3 hours fully charged


ADD-ONS(Sold Separately)
	SE2000iE Smart Inverter Generator
	100~240VAC, Max.1200W

	DSF/DS Series Solar Panels
	20.5V/41V, Max. 400W


 NOTE  

(1). The DC charger and Driving charger are optional equipment.
(2).Whether the product can be charged or discharged depends on the actual temperature of the battery pack. The maximum charging or discharging power is related to the ambient temperature and SOC of battery.
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